|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | | --- | | **Simulation of Foot Left**  **Date: Wednesday, April 9, 2025 Designer: Solidworks**  **Study name: Static 1**  **Analysis type: Static** | | Table of Contents  [Description 1](#_Toc195053343)  [Assumptions 2](#_Toc195053344)  [Model Information 2](#_Toc195053345)  [Study Properties 3](#_Toc195053346)  [Units 3](#_Toc195053347)  [Material Properties 4](#_Toc195053348)  [Loads and Fixtures 4](#_Toc195053349)  [Connector Definitions 5](#_Toc195053350)  [Interaction Information 5](#_Toc195053351)  [Mesh information 6](#_Toc195053352)  [Sensor Details 7](#_Toc195053353)  [Resultant Forces 7](#_Toc195053354)  [Beams 8](#_Toc195053355)  [Study Results 9](#_Toc195053356)  [Conclusion 11](#_Toc195053357) | |
| Description No Data |

|  |
| --- |
| Assumptions |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model Information  |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | |  |   ****Model name:** Foot Left**  ****Current Configuration:** Default** | | | | | ****Solid Bodies**** | | | | | ****Document Name and Reference**** | ****Treated As**** | ****Volumetric Properties**** | ****Document Path/Date Modified**** | | **Cut-Extrude1** | **Solid Body** | ****Mass:0.634575 kg****  ****Volume:0.000235028 m^3****  ****Density:2,700 kg/m^3****  ****Weight:6.21883 N**** | ****C:\Users\allen\Documents\GitHub\CAPSTONE\_LowerLimbExoskeleton\3D Redesign\Exoskeleton\Foot Left.SLDPRT****  **Apr 6 19:37:24 2025** | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Properties  |  |  | | --- | --- | | Study name | Static 1 | | Analysis type | Static | | Mesh type | Solid Mesh | | Thermal Effect: | On | | Thermal option | Include temperature loads | | Zero strain temperature | 298 Kelvin | | Include fluid pressure effects from SOLIDWORKS Flow Simulation | Off | | Solver type | Automatic | | Inplane Effect: | Off | | Soft Spring: | Off | | Inertial Relief: | Off | | Incompatible bonding options | Automatic | | Large displacement | On | | Compute free body forces | On | | Friction | Off | | Use Adaptive Method: | Off | | Result folder | SOLIDWORKS document (C:\Users\allen\Documents\GitHub\CAPSTONE\_LowerLimbExoskeleton\3D Redesign\Exoskeleton) | |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Units  |  |  | | --- | --- | | Unit system: | SI (MKS) | | Length/Displacement | mm | | Temperature | Kelvin | | Angular velocity | Rad/sec | | Pressure/Stress | N/m^2 | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Material Properties  |  |  |  | | --- | --- | --- | | ****Model Reference**** | ****Properties**** | ****Components**** | |  | |  |  | | --- | --- | | ****Name:**** | **6061 Alloy** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Max von Mises Stress** | | ****Yield strength:**** | **5.51485e+07 N/m^2** | | ****Tensile strength:**** | **1.24084e+08 N/m^2** | | ****Elastic modulus:**** | **6.9e+10 N/m^2** | | ****Poisson's ratio:**** | **0.33** | | ****Mass density:**** | **2,700 kg/m^3** | | ****Shear modulus:**** | **2.6e+10 N/m^2** | | ****Thermal expansion coefficient:**** | **2.4e-05 /Kelvin** | | **SolidBody 1(Cut-Extrude1)(Foot Left)** | | **Curve Data:N/A** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Loads and Fixtures**  | ****Fixture name**** | ****Fixture Image**** | ****Fixture Details**** | | --- | --- | --- | | **Fixed-1** |  | |  |  | | --- | --- | | Entities: | **1 face(s)** | | Type: | **Fixed Geometry** | | | ****Resultant Forces****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Reaction force(N)** | **-7.62939e-06** | **250** | **-7.15256e-06** | **250** | | **Reaction Moment(N.m)** | **0** | **0** | **0** | **0** | | | |  | ****Load name**** | ****Load Image**** | ****Load Details**** | | --- | --- | --- | | **Force-1** |  | |  |  | | --- | --- | | Entities: | **1 face(s)** | | Type: | **Apply normal force** | | Value: | **250 N** | | |

|  |
| --- |
| Connector Definitions No Data |

|  |
| --- |
| Interaction Information No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Mesh information  |  |  | | --- | --- | | Mesh type | Solid Mesh | | Mesher Used: | Blended curvature-based mesh | | Jacobian points for High quality mesh | 16 Points | | Maximum element size | 6.17297 mm | | Minimum element size | 6.17297 mm | | Mesh Quality | High |  Mesh information - Details  |  |  | | --- | --- | | Total Nodes | 17404 | | Total Elements | 10029 | | Maximum Aspect Ratio | 3.8626 | | % of elements with Aspect Ratio < 3 | 100 | | Percentage of elements with Aspect Ratio > 10 | 0 | | Percentage of distorted elements | 0 | | Time to complete mesh(hh;mm;ss): | 00:00:02 | | Computer name: | ENGRLEANDZ |  Mesh Quality Plots  | Name | Type | Min | Max | | --- | --- | --- | --- | | Quality1 | Mesh | - | - | | **Foot Left-Static 1-Quality-Quality1** | | | | |

|  |
| --- |
| Sensor Details No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Resultant ForcesReaction forces  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N | -7.62939e-06 | 250 | -7.15256e-06 | 250 |  Reaction Moments  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N.m | 0 | 0 | 0 | 0 | |
| Free body forces  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N | 0 | 0 | 0 | 0 |  Free body moments  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N.m | 0 | 0 | 0 | 0 | |

|  |
| --- |
| Beams No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Results  | Name | Type | Min | Max | | --- | --- | --- | --- | | Stress1 | VON: von Mises Stress | 7.928e+03N/m^2  Node: 2202 | 3.506e+07N/m^2  Node: 7166 | | **Foot Left-Static 1-Stress-Stress1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Displacement1 | URES: Resultant Displacement | 0.000e+00mm  Node: 13 | 4.179e-01mm  Node: 17183 | | **Foot Left-Static 1-Displacement-Displacement1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Strain1 | ESTRN: Equivalent Strain | 4.332e-07  Element: 6003 | 3.162e-04  Element: 1149 | | **Foot Left-Static 1-Strain-Strain1** | | | |  | Name | Type | | --- | --- | | Displacement1{1} | Deformed shape | | **Foot Left-Static 1-Displacement-Displacement1{1}** | | |

|  |
| --- |
| Conclusion |